IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Номер проекта"
Time stamp: "2021-12-22T09:54:25"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.20.44 - Exporter 21.4.0.0 - Alternate UI 21.4.0.0"
Application: "Autodesk Revit 2021 (RUS)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (RUS)"

People and organizations
  Person "anna1869@yandex.ru" of Organization (no name given)
  Owner history of Person "anna1869@yandex.ru" of Organization (no name given) | application "Autodesk Revit 2021 (RUS)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (RUS)" | change NOCHANGE | created 1631274812 (2021-09-10T11:53:32Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Номер проекта" | long name "Наименование проекта" | phase "П"
  IFCSITE "Default" | latitude 55° 44′ 57.789001″ | longitude 37° 38′ 4.304809″ | elevation above sea level 203500.
    IFCBUILDING "Наименование здания" | long name "Наименование здания" | postal address: "Адрес проекта", "55.7493858337402", "37.6345291137695"
      IFCBUILDINGSTOREY "Подвал" | long name "Подвал" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation -4200.
        contains 1683 elements
          461 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2421053", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2426306", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2433570" (+458 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2426240", "470_DKC_S5_Variable Angle Elbow 0-45:-:2970025", "470_DKC_S5_Variable Angle Elbow 0-45:-:3118360" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2466440", "470_DKC_S5_Variable Angle Elbow 0-45:-:2974546", "470_DKC_S5_Variable Angle Elbow 0-45:-:3052530" (+4 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          42 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2527953", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2528248", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2528299" (+39 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          45 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Типы трубопроводов:По умолчанию" | object type "Типы трубопроводов:По умолчанию" | names: "Типы трубопроводов:По умолчанию:2904831", "Типы трубопроводов:По умолчанию:2904835", "Типы трубопроводов:По умолчанию:2904839" (+42 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          31 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2969963", "470_DKC_S5_Variable Angle Elbow 0-45:-:3045474", "470_DKC_S5_Variable Angle Elbow 0-45:-:3051685" (+28 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          16 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2970909", "470_DKC_S5_Variable Angle Elbow 0-45:-:3048666", "470_DKC_S5_Variable Angle Elbow 0-45:-:3083902" (+13 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          183 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048015", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048207", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048568" (+180 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          183 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048016", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048208", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048569" (+180 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          185 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048017", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048209", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048570" (+182 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          185 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048018", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048210", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3048571" (+182 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3048521", "470_DKC_S5_Variable Angle Elbow 0-45:-:3048523" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3048717", "470_DKC_S5_Variable Angle Elbow 0-45:-:3048719" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          41 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053287", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053365", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3086479" (+38 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          41 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053288", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053366", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3086480" (+38 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          42 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053289", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053367", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3086481" (+39 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          42 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053290", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3053368", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3086482" (+39 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3053405", "470_DKC_S5_Variable Angle Elbow 0-45:-:3053407" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3053842", "470_DKC_S5_Variable Angle Elbow 0-45:-:3053844", "470_DKC_S5_Variable Angle Elbow 0-45:-:3054041" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3053911" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055169" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055187" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055254" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055256" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055835" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055845" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055865" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3055869" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3062064", "470_DKC_S5_Variable Angle Elbow 0-45:-:3063473", "470_DKC_S5_Variable Angle Elbow 0-45:-:3064096" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3062386" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3062388" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3064013", "470_DKC_S5_Variable Angle Elbow 0-45:-:3152152", "470_DKC_S5_Variable Angle Elbow 0-45:-:3152742" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3064094" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3064757" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          11 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3070392", "470_DKC_S5_Variable Angle Elbow 0-45:-:3086422", "470_DKC_S5_Variable Angle Elbow 0-45:-:3093178" (+8 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3083911", "470_DKC_S5_Variable Angle Elbow 0-45:-:3159073" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3084783", "470_DKC_S5_Variable Angle Elbow 0-45:-:3085144" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3085162" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3085165", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3142933", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3143272" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3086865", "470_DKC_S5_Variable Angle Elbow 0-45:-:3087130", "470_DKC_S5_Variable Angle Elbow 0-45:-:3162484" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3087222" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3087319", "470_DKC_S5_Variable Angle Elbow 0-45:-:3162188" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3089106", "470_DKC_S5_Variable Angle Elbow 0-45:-:3090888", "470_DKC_S5_Variable Angle Elbow 0-45:-:3162332" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неперфорированный:3091544" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3092201" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | object type "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | names: "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-:3104229" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3105286", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3105355", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3142972" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          10 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3109952", "470_DKC_S5_Variable Angle Elbow 0-45:-:3109954", "470_DKC_S5_Variable Angle Elbow 0-45:-:3110022" (+7 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3110044", "470_DKC_S5_CPO 45 horizontal angle:-:3110320", "470_DKC_S5_CPO 45 horizontal angle:-:3142889" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3110046" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3110126" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3110128", "470_DKC_S5_Variable Angle Elbow 0-45:-:3143464" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3110419" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:3110486", "470_DKC_S5_CPO 45 horizontal angle:-:3110527", "470_DKC_S5_CPO 45 horizontal angle:-:3110565" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3110770", "470_DKC_S5_Variable Angle Elbow 0-45:-:3110792", "470_DKC_S5_Variable Angle Elbow 0-45:-:3230963" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3114789" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3114793" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3123952", "470_DKC_S5_Variable Angle Elbow 0-45:-:3124734" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3124089", "470_DKC_S5_Variable Angle Elbow 0-45:-:3124715" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3125850", "470_DKC_S5_Variable Angle Elbow 0-45:-:3129390" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3127944" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3127945" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3142197", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3142535" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3142198", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3142536" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3143722" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3152395" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3152900" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3181812", "470_DKC_S5_Variable Angle Elbow 0-45:-:3181822", "470_DKC_S5_Variable Angle Elbow 0-45:-:3182023" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3182356", "470_DKC_S5_Variable Angle Elbow 0-45:-:3182370", "470_DKC_S5_Variable Angle Elbow 0-45:-:3182532" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3231374" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3252732", "470_DKC_S5_Variable Angle Elbow 0-45:-:3252734" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3252999" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3278704", "470_DKC_S5_Variable Angle Elbow 0-45:-:3278706" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3281692", "470_DKC_S5_Variable Angle Elbow 0-45:-:3281706" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3281778", "470_DKC_S5_Variable Angle Elbow 0-45:-:3281788" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3281824", "470_DKC_S5_Variable Angle Elbow 0-45:-:3281830" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3281967", "470_DKC_S5_Variable Angle Elbow 0-45:-:3282024" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3282078", "470_DKC_S5_Variable Angle Elbow 0-45:-:3282098" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3282110", "470_DKC_S5_Variable Angle Elbow 0-45:-:3282126" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3282158", "470_DKC_S5_Variable Angle Elbow 0-45:-:3282164" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3282180", "470_DKC_S5_Variable Angle Elbow 0-45:-:3282438" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3283213", "470_DKC_S5_Variable Angle Elbow 0-45:-:3283229" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3283243", "470_DKC_S5_Variable Angle Elbow 0-45:-:3283245" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3283451" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3283573" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3283575" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_L5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_L5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_L5_Ladder tray:3283913", "Кабельный лоток с соединительными деталями:DKC_L5_Ladder tray:3284231", "Кабельный лоток с соединительными деталями:DKC_L5_Ladder tray:3287886" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3284972", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286033", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286054" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3284973", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286034", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286055" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3284974", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286035", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286056" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3284975", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286036", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3286057" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:3285897" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:3286253" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3286346" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3286528" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3286894" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3287032", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3287103", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:3287111" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3287129" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 01" | long name "Этаж 01" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 0.
        contains 1215 elements
          310 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2122202", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2122203", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2126544" (+307 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2379958", "470_DKC_S5_Variable Angle Elbow 0-45:-:2452095" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2379971", "470_DKC_S5_Variable Angle Elbow 0-45:-:2388807" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование" | object type "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование" | names: "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование:2379973", "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование:2388785" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | object type "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | names: "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2379974", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388786", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2391493" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | object type "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | names: "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2379975", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388787", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2391494" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | object type "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | names: "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2379996", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2379997", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388798" (+6 more) | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | object type "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | names: "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-:2380005", "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-:2388673", "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-:2391380" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2380010", "470_DKC_S5_Variable Angle Elbow 0-45:-:2389501" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | object type "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | names: "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера:2388519", "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера:2390093" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | object type "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | names: "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388520", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388530", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388531" (+6 more) | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | object type "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | names: "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2388521", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2390095", "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2391524" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TD vertical T-tapper:-" | object type "470_DKC_S5_TD vertical T-tapper:-" | names: "470_DKC_S5_TD vertical T-tapper:-:2388546", "470_DKC_S5_TD vertical T-tapper:-:2388559", "470_DKC_S5_TD vertical T-tapper:-:2388697" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          158 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2388651", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2393156", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2401734" (+155 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          158 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2388652", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2393157", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2401735" (+155 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          160 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2388653", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2393158", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2401736" (+157 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          160 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2388654", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2393159", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2401737" (+157 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2389988", "470_DKC_S5_Variable Angle Elbow 0-45:-:2389990", "470_DKC_S5_Variable Angle Elbow 0-45:-:2452093" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование" | object type "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование" | names: "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование:2391492" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | object type "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | names: "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера:2391522" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2393183", "470_DKC_S5_Variable Angle Elbow 0-45:-:2490576", "470_DKC_S5_Variable Angle Elbow 0-45:-:2490724" (+4 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2393227", "470_DKC_S5_Variable Angle Elbow 0-45:-:2875018" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2394582", "470_DKC_S5_DPT T-tapper:-:2418513" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2395024", "470_DKC_S5_Variable Angle Elbow 0-45:-:2500845" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2395038", "470_DKC_S5_Variable Angle Elbow 0-45:-:2500919" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2408392", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2408552" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2408393", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2408553" | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2426620", "470_DKC_S5_Variable Angle Elbow 0-45:-:2490508", "470_DKC_S5_Variable Angle Elbow 0-45:-:2501250" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2460269" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2460338", "470_DKC_S5_Variable Angle Elbow 0-45:-:2460588" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2463730", "470_DKC_S5_CPO 45 horizontal angle:-:2463732", "470_DKC_S5_CPO 45 horizontal angle:-:2466129" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          38 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465736", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465795", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465816" (+35 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          38 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465737", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465796", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465817" (+35 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          38 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465738", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465797", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465818" (+35 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          38 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465739", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465798", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2465819" (+35 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2475345", "470_DKC_S5_CPO 45 horizontal angle:-:2475375" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2479641", "470_DKC_S5_Variable Angle Elbow 0-45:-:2480228" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2479685", "470_DKC_S5_Variable Angle Elbow 0-45:-:2480642" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2480754" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2485382", "470_DKC_S5_Variable Angle Elbow 0-45:-:2491099" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2500517" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2500630" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2514450", "470_DKC_S5_Variable Angle Elbow 0-45:-:2514642", "470_DKC_S5_Variable Angle Elbow 0-45:-:2514847" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2514452" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2518987" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2519247", "470_DKC_S5_Variable Angle Elbow 0-45:-:2519264" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | object type "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | names: "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера:2521850" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | object type "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | names: "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ:2521893" | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2522168" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2522752" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2525279", "470_DKC_S5_Variable Angle Elbow 0-45:-:2525319", "470_DKC_S5_Variable Angle Elbow 0-45:-:2873955" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551004", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551005", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551006" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2808928", "470_DKC_S5_Variable Angle Elbow 0-45:-:2808946" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2825455" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2875338" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 02" | long name "Этаж 02" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 4200.
        contains 789 elements
          409 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1927267", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1930797", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1981030" (+406 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2303320" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2303516", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2303584" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2303668", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2303672" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2304692", "470_DKC_S5_Variable Angle Elbow 0-45:-:2304704", "470_DKC_S5_Variable Angle Elbow 0-45:-:2306715" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2306198", "470_DKC_S5_Variable Angle Elbow 0-45:-:2306717" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2306800" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2307716" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2307840", "470_DKC_S5_Variable Angle Elbow 0-45:-:2335607", "470_DKC_S5_Variable Angle Elbow 0-45:-:2336103" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2308464", "470_DKC_S5_Variable Angle Elbow 0-45:-:2308474" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2309496", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2309502" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2309562", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2309845", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2310118" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2309783" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2310085", "470_DKC_S5_Variable Angle Elbow 0-45:-:2378930" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2325990" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2325993", "470_DKC_S5_Variable Angle Elbow 0-45:-:2325997" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2326001", "470_DKC_S5_Variable Angle Elbow 0-45:-:2326005" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2326009" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2326013" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2335611" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2335622", "470_DKC_S5_CD 90 external vertical angle:-:2335630" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2335632", "470_DKC_S5_CS 90 internal vertical angle:-:2344895" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2335636", "470_DKC_S5_CD 90 external vertical angle:-:2335645" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2335641", "470_DKC_S5_CS 90 internal vertical angle:-:2335649" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2335653" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2335677", "470_DKC_S5_Variable Angle Elbow 0-45:-:2335784", "470_DKC_S5_Variable Angle Elbow 0-45:-:2982614" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2335743" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          14 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2335905", "470_DKC_S5_Variable Angle Elbow 0-45:-:2377078", "470_DKC_S5_Variable Angle Elbow 0-45:-:2984551" (+11 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2336107" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2336846", "470_DKC_S5_DPT T-tapper:-:2376336" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2339947" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          15 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2340219", "470_DKC_S5_Variable Angle Elbow 0-45:-:2376928", "470_DKC_S5_Variable Angle Elbow 0-45:-:2985815" (+12 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2340653", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2340669" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2362096" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2362114", "470_DKC_S5_Variable Angle Elbow 0-45:-:2362123" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2362178", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992976", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3061192" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2362189" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2362191" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2362195" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2362197" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2362204" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2365907", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2987479" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2376812", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2376930", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3000950" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377036", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377080", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3000904" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377201", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3000879" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377589", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377956" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377881", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2377958" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2378651", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2378759", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2378839" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2378761", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2378784", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2378891" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2378782" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2379050", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2379125", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2379574" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2379497", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2379503", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2379576" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551009", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551010", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551011" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977468", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977482", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980216" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977510", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977512", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977617" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977609" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977668", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977708", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977714" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977687", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977689" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977799", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977801" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977839", "470_DKC_S5_Variable Angle Elbow 0-45:-:3030181" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977859", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977861" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977900", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977914" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2977938", "470_DKC_S5_Variable Angle Elbow 0-45:-:2977940" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2978913", "470_DKC_S5_Variable Angle Elbow 0-45:-:2978919", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981994" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2978933", "470_DKC_S5_Variable Angle Elbow 0-45:-:2978935" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2978974", "470_DKC_S5_Variable Angle Elbow 0-45:-:2978980" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2979116", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979124" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2979200", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979210", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979251" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2979224", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979226" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2979561", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979563" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2979616", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979622" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2979634", "470_DKC_S5_Variable Angle Elbow 0-45:-:2979648" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2980306", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980308" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2980361", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980367", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980483" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2980423", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980425", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981323" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2980503", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980505" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2980580", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980586" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2980622", "470_DKC_S5_Variable Angle Elbow 0-45:-:2980624" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981177", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981183" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981199", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981201" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981253", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981261" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981275", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981277" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981343", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981345" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981512", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981523" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981548", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981554" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981646", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981648" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2981955", "470_DKC_S5_Variable Angle Elbow 0-45:-:2981961" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2982026", "470_DKC_S5_Variable Angle Elbow 0-45:-:2982032" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2982056", "470_DKC_S5_Variable Angle Elbow 0-45:-:2982062" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2982142", "470_DKC_S5_Variable Angle Elbow 0-45:-:2982148" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2983433", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2983688" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2983611" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2983682" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2984668", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2984728", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2985016" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2984859", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2984862", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2985019" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986026", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986086", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986704" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986652", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986654", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986708" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2986792", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2987122", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3005595" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2990019", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2990021" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2990093" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2990751" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2990818" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2990826" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2990871", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2990886" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2991346" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2991522", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2991524" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2991920", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992091", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992350" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992089", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992348", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992371" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992729", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2992733" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2998831", "470_DKC_S5_Variable Angle Elbow 0-45:-:2998839" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2999142", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2999157" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2999590" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2999845", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2999848" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3002179" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3002277", "470_DKC_S5_DPT T-tapper:-:3003847" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3003168", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3067582" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3003515", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3003592" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3004365", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3004368" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3004796", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3004843" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3005039", "470_DKC_S5_DPT T-tapper:-:3036050" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3006196", "470_DKC_S5_Variable Angle Elbow 0-45:-:3006198" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3022286", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3022403" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3022477", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3078876" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3028322", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3028954", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3060133" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3029681", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3060053" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3029901", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3029905" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3030183", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3030206" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3039741", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3039744" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3039794", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3039798" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3045578", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3045580", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3045585" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3045590" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3045608", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3057064" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3045623" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3054538", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3054561", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3056160" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3054546" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3054548" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Перфорированный" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Перфорированный" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Перфорированный:3058161" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3058204", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3059726", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3060114" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3059860" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3059993" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:3059996" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3060055" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3060135", "470_DKC_S5_Variable Angle Elbow 0-45:-:3060184" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3066256", "470_DKC_S5_Variable Angle Elbow 0-45:-:3066266", "470_DKC_S5_Variable Angle Elbow 0-45:-:3067258" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3067206", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3067208" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3067375", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:3067421" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3331905", "470_DKC_S5_Variable Angle Elbow 0-45:-:3331919" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3332202", "470_DKC_S5_Variable Angle Elbow 0-45:-:3332208" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:3332332" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:3332444", "470_DKC_S5_Variable Angle Elbow 0-45:-:3335404" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332724", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332745", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3334373" (+2 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332725", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332746", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3334374" (+2 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332726", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332747", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3334375" (+2 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332727", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3332748", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:3334376" (+2 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 03" | long name "Этаж 03" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 8100.
        contains 1293 elements
          453 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Sheet tray:962603", "Кабельный лоток с соединительными деталями:DKC_G5_Sheet tray:962654", "Кабельный лоток с соединительными деталями:DKC_G5_Sheet tray:964799" (+450 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:962967", "470_DKC_S5_DPT T-tapper:-:964878" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:1850342", "470_DKC_S5_CDV 90 external vertical angle:-:1850347", "470_DKC_S5_CDV 90 external vertical angle:-:1882854" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:1851440" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:1851930", "470_DKC_S5_CDV 90 external vertical angle:-:1851934", "470_DKC_S5_CDV 90 external vertical angle:-:1852154" (+9 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:1867571", "470_DKC_G5_Sheet horizontal bend:-:1876359", "470_DKC_G5_Sheet horizontal bend:-:1876387" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          11 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_F5_Mesh horizontal angle:At right angles" | object type "470_DKC_F5_Mesh horizontal angle:At right angles" | names: "470_DKC_F5_Mesh horizontal angle:At right angles:1867740", "470_DKC_F5_Mesh horizontal angle:At right angles:1868145", "470_DKC_F5_Mesh horizontal angle:At right angles:1868525" (+8 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_F5_Mesh horizontal angle:At right angles" | object type "470_DKC_F5_Mesh horizontal angle:At right angles" | names: "470_DKC_F5_Mesh horizontal angle:At right angles:1868924", "470_DKC_F5_Mesh horizontal angle:At right angles:1868998", "470_DKC_F5_Mesh horizontal angle:At right angles:1876158" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:1869059", "470_DKC_G5_Sheet horizontal bend:-:1869064" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:1869577", "470_DKC_S5_CDV 90 external vertical angle:-:1869581", "470_DKC_S5_CDV 90 external vertical angle:-:1869801" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:1869950", "470_DKC_S5_CDV 90 external vertical angle:-:1869954", "470_DKC_S5_CDV 90 external vertical angle:-:1872128" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:1871861" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1875832", "470_DKC_S5_Variable Angle Elbow 0-45:-:1891301" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:1876837", "470_DKC_G5_Sheet horizontal bend:-:1888064" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1881395", "470_DKC_S5_Variable Angle Elbow 0-45:-:2120214" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1882914", "470_DKC_S5_Variable Angle Elbow 0-45:-:1882918" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1883117", "470_DKC_S5_Variable Angle Elbow 0-45:-:1883313", "470_DKC_S5_Variable Angle Elbow 0-45:-:1883343" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1884651", "470_DKC_S5_Variable Angle Elbow 0-45:-:1884655" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1884686", "470_DKC_S5_Variable Angle Elbow 0-45:-:2133846" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1884726", "470_DKC_S5_Variable Angle Elbow 0-45:-:2133746" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1884816", "470_DKC_S5_Variable Angle Elbow 0-45:-:1884818" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1884872", "470_DKC_S5_Variable Angle Elbow 0-45:-:1884876" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1884936", "470_DKC_S5_Variable Angle Elbow 0-45:-:1884940" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:1887875" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1890197" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1890245", "470_DKC_S5_Variable Angle Elbow 0-45:-:1895711", "470_DKC_S5_Variable Angle Elbow 0-45:-:1895832" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1891111", "470_DKC_S5_Variable Angle Elbow 0-45:-:1891123" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1891166", "470_DKC_S5_Variable Angle Elbow 0-45:-:1891178" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1911616" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:1911622" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:1940417", "470_DKC_G5_Sheet horizontal bend:-:1960420" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TSS tapper-cover (flat):-" | object type "470_DKC_S5_TSS tapper-cover (flat):-" | names: "470_DKC_S5_TSS tapper-cover (flat):-:2223545", "470_DKC_S5_TSS tapper-cover (flat):-:2223562" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TSS tapper-cover (flat):-" | object type "470_DKC_S5_TSS tapper-cover (flat):-" | names: "470_DKC_S5_TSS tapper-cover (flat):-:2223628", "470_DKC_S5_TSS tapper-cover (flat):-:2223644" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>"); "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          64 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229872", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229979", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229999" (+61 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          64 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229873", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229980", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2230000" (+61 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          64 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229874", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229981", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2230001" (+61 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          64 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229875", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2229982", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2230002" (+61 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2230351" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2233227" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          104 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237259", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237293", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237375" (+101 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          104 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237260", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237294", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237376" (+101 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          104 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237261", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237295", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237377" (+101 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          104 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237262", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237296", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2237378" (+101 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:2293660", "470_DKC_S5_CDV 90 external vertical angle:-:2293815" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2295133", "470_DKC_G5_Sheet horizontal bend:-:2295703", "470_DKC_G5_Sheet horizontal bend:-:2296393" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          12 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2295607", "470_DKC_G5_Sheet horizontal bend:-:2295632", "470_DKC_G5_Sheet horizontal bend:-:2295651" (+9 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Переход канального лотка:Переход канального лотка" | object type "Переход канального лотка:Переход канального лотка" | names: "Переход канального лотка:Переход канального лотка:2295702" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:2297033" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2297771", "470_DKC_G5_Sheet horizontal bend:-:2297974" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2297838", "470_DKC_G5_Sheet horizontal bend:-:2297909", "470_DKC_G5_Sheet horizontal bend:-:2298418" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2324738", "470_DKC_G5_Sheet horizontal bend:-:2324788", "470_DKC_G5_Sheet horizontal bend:-:2324827" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet reducer:-" | object type "470_DKC_G5_Sheet reducer:-" | names: "470_DKC_G5_Sheet reducer:-:2369097" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2373159", "470_DKC_G5_Sheet horizontal bend:-:2375743" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2374201" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2374207" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2374370", "470_DKC_S5_Variable Angle Elbow 0-45:-:2374388", "470_DKC_S5_Variable Angle Elbow 0-45:-:2374504" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2374463" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2374670", "470_DKC_G5_Sheet horizontal bend:-:2374783" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2375809" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2376019", "470_DKC_G5_Sheet horizontal bend:-:2376177", "470_DKC_G5_Sheet horizontal bend:-:2376327" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2387958", "470_DKC_G5_Sheet horizontal bend:-:2388016" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:2388013" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:2388094", "470_DKC_S5_CDV 90 external vertical angle:-:2388116" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | object type "470_DKC_G5_Sheet horizontal bend:-" | names: "470_DKC_G5_Sheet horizontal bend:-:2388097", "470_DKC_G5_Sheet horizontal bend:-:2388119", "470_DKC_G5_Sheet horizontal bend:-:2388176" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2421166" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2421209", "470_DKC_S5_Variable Angle Elbow 0-45:-:2421252" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551013", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551014", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551015" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 04" | long name "Этаж 04" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 12000.
        contains 671 elements
          186 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1914518", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1914852", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1916439" (+183 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2017393", "470_DKC_S5_DPT T-tapper:-:2018157" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          73 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2018114", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023758", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023808" (+70 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          73 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2018115", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023759", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023809" (+70 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          77 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2018116", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023760", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023810" (+74 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          77 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2018117", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023761", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2023811" (+74 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2023350", "470_DKC_S5_DPT T-tapper:-:2033673", "470_DKC_S5_DPT T-tapper:-:2241654" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2023401", "470_DKC_S5_Variable Angle Elbow 0-45:-:2286277", "470_DKC_S5_Variable Angle Elbow 0-45:-:2299702" (+4 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2024105", "470_DKC_S5_DPT T-tapper:-:2033644" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2025016", "470_DKC_S5_Variable Angle Elbow 0-45:-:2245375", "470_DKC_S5_Variable Angle Elbow 0-45:-:2285887" (+4 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          30 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025358", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025554", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025979" (+27 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          30 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025359", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025555", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025980" (+27 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          30 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025360", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025556", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025981" (+27 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          30 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025361", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025557", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2025982" (+27 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2025402", "470_DKC_S5_Variable Angle Elbow 0-45:-:2026105", "470_DKC_S5_Variable Angle Elbow 0-45:-:2244521" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2025813" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2026005" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2026057", "470_DKC_S5_RRC_RRS_RRD adapter:-:2303420" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2030446", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2030468", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2030509" (+1 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2030447", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2030469", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2030510" (+1 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2033856", "470_DKC_S5_CPO 45 horizontal angle:-:2053421" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2053247" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TSS tapper-cover (flat):-" | object type "470_DKC_S5_TSS tapper-cover (flat):-" | names: "470_DKC_S5_TSS tapper-cover (flat):-:2234526", "470_DKC_S5_TSS tapper-cover (flat):-:2238648", "470_DKC_S5_TSS tapper-cover (flat):-:2246592" (+1 more) | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:2239999", "470_DKC_S5_CDV 90 external vertical angle:-:2264469" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2242391" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2244755", "470_DKC_S5_Variable Angle Elbow 0-45:-:2244861", "470_DKC_S5_Variable Angle Elbow 0-45:-:2284534" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2247362", "470_DKC_S5_CPO 45 horizontal angle:-:2263092" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2301302", "470_DKC_S5_Variable Angle Elbow 0-45:-:2301304", "470_DKC_S5_Variable Angle Elbow 0-45:-:2301346" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2303418", "470_DKC_S5_Variable Angle Elbow 0-45:-:2303423" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551017", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551018", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551019" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 05" | long name "Этаж 05" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 15900.
        contains 905 elements
          333 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1957976", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1958243", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:1958655" (+330 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2005070", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2005265", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2354398" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2005078", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2005270", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2010734" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2005167", "470_DKC_S5_Variable Angle Elbow 0-45:-:2005169" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2005173", "470_DKC_S5_Variable Angle Elbow 0-45:-:2005175" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2005179", "470_DKC_S5_Variable Angle Elbow 0-45:-:2005181" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2005185", "470_DKC_S5_Variable Angle Elbow 0-45:-:2005187" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2005191", "470_DKC_S5_Variable Angle Elbow 0-45:-:2005193" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2005197", "470_DKC_S5_Variable Angle Elbow 0-45:-:2005199" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2010694" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2010698" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2010738", "470_DKC_S5_Variable Angle Elbow 0-45:-:2010740", "470_DKC_S5_Variable Angle Elbow 0-45:-:2010770" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2010776", "470_DKC_S5_Variable Angle Elbow 0-45:-:2010780" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2010784", "470_DKC_S5_Variable Angle Elbow 0-45:-:2010786" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2010790", "470_DKC_S5_Variable Angle Elbow 0-45:-:2010794", "470_DKC_S5_Variable Angle Elbow 0-45:-:2010797" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2012188", "470_DKC_S5_CD 90 external vertical angle:-:2012195" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2012257", "470_DKC_S5_CD 90 external vertical angle:-:2012264" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2012330", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2012337" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2012364", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2012368" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2013408" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2013413" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2013508" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2013549", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2013576", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2018820" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2015038" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2015043" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2015065" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2015093" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2015120" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2018816" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2018818" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2021982", "470_DKC_S5_Variable Angle Elbow 0-45:-:2021985", "470_DKC_S5_Variable Angle Elbow 0-45:-:2022025" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2021991", "470_DKC_S5_Variable Angle Elbow 0-45:-:2022041" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2021995", "470_DKC_S5_Variable Angle Elbow 0-45:-:2022051" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022003", "470_DKC_S5_Variable Angle Elbow 0-45:-:2078278" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022009", "470_DKC_S5_Variable Angle Elbow 0-45:-:2022071" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022151", "470_DKC_S5_Variable Angle Elbow 0-45:-:2022166", "470_DKC_S5_Variable Angle Elbow 0-45:-:2060350" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022156", "470_DKC_S5_Variable Angle Elbow 0-45:-:2022162", "470_DKC_S5_Variable Angle Elbow 0-45:-:2060374" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022171", "470_DKC_S5_Variable Angle Elbow 0-45:-:2060326", "470_DKC_S5_Variable Angle Elbow 0-45:-:2081630" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022176", "470_DKC_S5_Variable Angle Elbow 0-45:-:2061222", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082070" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2022181", "470_DKC_S5_Variable Angle Elbow 0-45:-:2061180", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082116" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2040268" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2041234", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2041257", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2041261" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2041328" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2044383" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2054271", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2054294", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2082655" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2055593", "470_DKC_S5_Variable Angle Elbow 0-45:-:2055595" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2055667", "470_DKC_S5_Variable Angle Elbow 0-45:-:2055697" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2055733" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2055760" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2056072", "470_DKC_S5_Variable Angle Elbow 0-45:-:2056074" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2056102", "470_DKC_S5_Variable Angle Elbow 0-45:-:2056129" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2056155" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2056424" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2056458" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2056462" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2058036" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2058135" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2058230" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2058284" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058463", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058465" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058492", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058494", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058671" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058523", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058525", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058594" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058695", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058697" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058719", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058721", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058793" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058743", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058745", "470_DKC_S5_Variable Angle Elbow 0-45:-:2058765" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2058763" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2058789" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2060097" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2060601" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2061677" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2062462" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2062728" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2062754" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2062812" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2062834" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2062880" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2062884" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2062912" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2076986" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2076992" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2076994" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2077003", "470_DKC_S5_Variable Angle Elbow 0-45:-:2077005" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2077009" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2077011" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2077013" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2077068" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2077073" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2077075" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2077081" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2078071", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2078600" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2078131", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2078618" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2078280" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2078405", "470_DKC_S5_CD 90 external vertical angle:-:2102102" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2080842", "470_DKC_S5_Variable Angle Elbow 0-45:-:2080844" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2080879" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2080881", "470_DKC_S5_Variable Angle Elbow 0-45:-:2081401", "470_DKC_S5_Variable Angle Elbow 0-45:-:2081403" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2081438", "470_DKC_S5_Variable Angle Elbow 0-45:-:2081440", "470_DKC_S5_Variable Angle Elbow 0-45:-:2081461" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2081953", "470_DKC_S5_Variable Angle Elbow 0-45:-:2081955" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2082023", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082025" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2082510", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082512" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2082545", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082588", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082758" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2082625", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082658", "470_DKC_S5_Variable Angle Elbow 0-45:-:2082686" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2083011" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2083062" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2083259", "470_DKC_S5_Variable Angle Elbow 0-45:-:2083261" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2083305", "470_DKC_S5_Variable Angle Elbow 0-45:-:2083315" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2085381" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2085784", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2085788", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2085811" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2086849" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2086855" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2097541" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2097620", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2102191" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2097647", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2097653" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2102075" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2102122" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2102128" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2102211", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2102215" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2102245", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный:2102249" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2102296" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Перфорированный" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Перфорированный" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Перфорированный:2354401" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          27 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354403", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354423", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354442" (+24 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          27 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354404", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354424", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354443" (+24 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          27 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354405", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354425", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354444" (+24 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          27 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354406", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354426", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354445" (+24 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          59 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354663", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354683", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354703" (+56 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          59 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354664", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354684", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354704" (+56 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          59 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354665", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354685", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354705" (+56 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          59 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354666", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354686", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2354706" (+56 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          4 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551021", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551022", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551023" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 06" | long name "Этаж 06" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 19800.
        contains 503 elements
          256 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2078952", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2086940", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2102344" (+253 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2130542" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134198", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134206" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134213", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134227", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134228" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134216", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134222", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2134226" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          27 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2134229", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2141002", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2141179" (+24 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный наружный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный наружный_Минимальный размер:Неспецифицируемый:2134234", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неспецифицируемый:2134260", "ADSK_Поворот вертикальный наружный_Минимальный размер:Неспецифицируемый:2134262" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2139706" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2139709", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325910" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          9 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2141325", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2148113", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2148245" (+6 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          23 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2141407", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2147458", "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2147522" (+20 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147496", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147499", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147506" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147524", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147526", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2148567" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147535", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147539", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2147589" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2148188", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2148247" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2149466", "470_DKC_S5_Variable Angle Elbow 0-45:-:2149572", "470_DKC_S5_Variable Angle Elbow 0-45:-:2149974" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2149647", "470_DKC_S5_Variable Angle Elbow 0-45:-:2149771", "470_DKC_S5_Variable Angle Elbow 0-45:-:2149818" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2149924" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2150886", "470_DKC_S5_Variable Angle Elbow 0-45:-:2151038", "470_DKC_S5_Variable Angle Elbow 0-45:-:2151330" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2150923", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2151040", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2151332" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2151393", "470_DKC_S5_Variable Angle Elbow 0-45:-:2151766", "470_DKC_S5_Variable Angle Elbow 0-45:-:2152020" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2151395", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2151768", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2151831" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2151474" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2151522", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2217121" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2153690", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156419" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2153771" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2153779" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154018", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154320", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154342" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154251", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154770", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2155224" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154291", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154380", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2154414" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156414", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156443" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156428" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156441", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2164027" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156449" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2156538", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2253226" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2161224", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2161318", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2167517" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2161411", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2223275" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2161731", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2164550" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2164535", "470_DKC_S5_DPT T-tapper:-:2166232", "470_DKC_S5_DPT T-tapper:-:2167439" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2165121", "470_DKC_S5_DPT T-tapper:-:2173463" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2165156" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2165316" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          7 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2166072", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2166186", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2167161" (+4 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2166913", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2166934", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2167602" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2167483" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2167637" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2168647", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2216850" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2169103", "470_DKC_S5_Variable Angle Elbow 0-45:-:2169117", "470_DKC_S5_Variable Angle Elbow 0-45:-:2169155" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2170337" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TDS vertical side T-tapper:-" | object type "470_DKC_S5_TDS vertical side T-tapper:-" | names: "470_DKC_S5_TDS vertical side T-tapper:-:2170806", "470_DKC_S5_TDS vertical side T-tapper:-:2172103" | material: materials ("Предупреждение", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2174058", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2174061" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2174167" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195577", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195743", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195745" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195761" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195794", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195795", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195830" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195898", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2195929" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | object type "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | names: "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-:2213723" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | object type "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | names: "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-:2217217" | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | object type "470_DKC_S5_CDV 90 external vertical angle:-" | names: "470_DKC_S5_CDV 90 external vertical angle:-:2220143" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2249620", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2252731" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2249888", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2249892" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250075", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250145" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый:2250141" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250246", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2252087" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250391", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251813" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250454", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251732" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250503", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2250506" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251621", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251627" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251718", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251777", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2251858" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2252446", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2252449" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2252654", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2252657" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2253202" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325911" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325918" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325923" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325925" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325936" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325938" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325940", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2495300" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325946" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2325948" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2495091", "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2495173" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2495093" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | object type "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | names: "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый:2495302" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2527833" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551025", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551026", "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551027" (+2 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Этаж 07" | long name "Этаж 07" | object type "Уровень:ADSK_Стрелка_Проектная_Вверх_Имя уровня" | elevation 24000.
        contains 920 elements
          285 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | object type "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | names: "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2466640", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2466661", "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray:2466716" (+282 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          25 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2466726", "470_DKC_S5_Variable Angle Elbow 0-45:-:2466732", "470_DKC_S5_Variable Angle Elbow 0-45:-:2467069" (+22 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2478830", "470_DKC_S5_Variable Angle Elbow 0-45:-:2478833", "470_DKC_S5_Variable Angle Elbow 0-45:-:2478836" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2478832", "470_DKC_S5_CPO 45 horizontal angle:-:2478835", "470_DKC_S5_CPO 45 horizontal angle:-:2478842" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DL T-tapper:-" | object type "470_DKC_S5_DL T-tapper:-" | names: "470_DKC_S5_DL T-tapper:-:2478843" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          82 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478852", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478872", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478923" (+79 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          82 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478853", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478873", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478924" (+79 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          82 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478854", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478874", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478925" (+79 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          82 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478855", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478875", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2478926" (+79 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2478892", "470_DKC_S5_CPO 45 horizontal angle:-:2844777", "470_DKC_S5_CPO 45 horizontal angle:-:2844798" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2478911", "470_DKC_S5_Variable Angle Elbow 0-45:-:2478913" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2542257", "470_DKC_S5_Variable Angle Elbow 0-45:-:2542772" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2542388" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2545155", "470_DKC_S5_Variable Angle Elbow 0-45:-:2546257" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2545706", "470_DKC_S5_Variable Angle Elbow 0-45:-:2545708" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2545767", "470_DKC_S5_Variable Angle Elbow 0-45:-:2545769" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2548361", "470_DKC_S5_Variable Angle Elbow 0-45:-:2548380", "470_DKC_S5_Variable Angle Elbow 0-45:-:2548399" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          42 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548719", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548741", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548801" (+39 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          42 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548720", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548742", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548802" (+39 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          42 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548721", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548743", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548803" (+39 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          42 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | object type "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | names: "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548722", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548744", "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС:2548804" (+39 more) | material: "G - Горячее цинкование" | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          1 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | object type "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | names: "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray:2551029" | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2842547", "470_DKC_S5_Variable Angle Elbow 0-45:-:2842549" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2842573", "470_DKC_S5_Variable Angle Elbow 0-45:-:2842575" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2843146", "470_DKC_S5_RRC_RRS_RRD adapter:-:2870522" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2843163", "470_DKC_S5_DPT T-tapper:-:2852161", "470_DKC_S5_DPT T-tapper:-:2868746" (+1 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2845831", "470_DKC_S5_Variable Angle Elbow 0-45:-:2845927", "470_DKC_S5_Variable Angle Elbow 0-45:-:2845929" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          8 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | object type "470_DKC_S5_CPO 45 horizontal angle:-" | names: "470_DKC_S5_CPO 45 horizontal angle:-:2847300", "470_DKC_S5_CPO 45 horizontal angle:-:2847339", "470_DKC_S5_CPO 45 horizontal angle:-:2847378" (+5 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          5 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2852236", "470_DKC_S5_Variable Angle Elbow 0-45:-:2917254", "470_DKC_S5_Variable Angle Elbow 0-45:-:2926114" (+2 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2852405", "470_DKC_S5_RRC_RRS_RRD adapter:-:2868933", "470_DKC_S5_RRC_RRS_RRD adapter:-:2910067" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | object type "470_DKC_S5_DPT T-tapper:-" | names: "470_DKC_S5_DPT T-tapper:-:2854476", "470_DKC_S5_DPT T-tapper:-:2912632" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          6 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2870161", "470_DKC_S5_Variable Angle Elbow 0-45:-:2870242", "470_DKC_S5_Variable Angle Elbow 0-45:-:2870365" (+3 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2870701", "470_DKC_S5_Variable Angle Elbow 0-45:-:2870703" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2870803", "470_DKC_S5_Variable Angle Elbow 0-45:-:2917375" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          11 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2871558", "470_DKC_S5_Variable Angle Elbow 0-45:-:2871586", "470_DKC_S5_Variable Angle Elbow 0-45:-:2910393" (+8 more) | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2888706", "470_DKC_S5_Variable Angle Elbow 0-45:-:2888708" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2913770", "470_DKC_S5_Variable Angle Elbow 0-45:-:2913772" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2914841", "470_DKC_S5_Variable Angle Elbow 0-45:-:2914895" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2914965" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2915235", "470_DKC_S5_Variable Angle Elbow 0-45:-:2916496" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2916418" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2916669" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2916695" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2916718" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2917659" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2917665" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2917695" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2917703" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | object type "470_DKC_S5_CD 90 external vertical angle:-" | names: "470_DKC_S5_CD 90 external vertical angle:-:2917726" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | object type "470_DKC_S5_CS 90 internal vertical angle:-" | names: "470_DKC_S5_CS 90 internal vertical angle:-:2917730" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2930621", "470_DKC_S5_Variable Angle Elbow 0-45:-:2930623" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2930648", "470_DKC_S5_Variable Angle Elbow 0-45:-:2930650" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2930671", "470_DKC_S5_Variable Angle Elbow 0-45:-:2930673" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | object type "470_DKC_S5_Variable Angle Elbow 0-45:-" | names: "470_DKC_S5_Variable Angle Elbow 0-45:-:2945176", "470_DKC_S5_Variable Angle Elbow 0-45:-:2945178" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2948618" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2948624" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | object type "470_DKC_S5_RRC_RRS_RRD adapter:-" | names: "470_DKC_S5_RRC_RRS_RRD adapter:-:2948630" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff

Types
  IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_S5_Sheet tray" | CABLETRAYSEGMENT | 2240 occurrences
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 7 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Ladder tray" | CABLETRAYSEGMENT | 68 occurrences
  IFCPIPESEGMENTTYPE "Типы трубопроводов:По умолчанию" | 45 occurrences
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 38 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 16 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 587 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 587 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 595 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 595 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 319 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 319 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 320 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 320 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 13 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 31 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неперфорированный" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>")
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 10 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 1 occurrence | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 1 occurrence | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 8 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 8 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_L5_Ladder tray" | CABLETRAYSEGMENT | 4 occurrences
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 3 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 3 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 3 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - ПШС:OSTEC_U - ЛН, ЛП - ПШС" | 3 occurrences | material: "G - Горячее цинкование" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование" | 2 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | 3 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | 3 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | 9 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | 3 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>")
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | 2 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | 9 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | 3 occurrences | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TD vertical T-tapper:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГРп - Тройник:G - Горячее цинкование" | 1 occurrence | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | 1 occurrence | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "OSTEC_CT - ЛН, ЛП - ОГп - Тройник:ZS - Цинкование по методу Сендзимера" | 1 occurrence | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "OSTEC_U - ЛН, ЛП - СЛУ:OSTEC_U - ЛН, ЛП - СЛУ" | 1 occurrence | material: "ZS - Цинкование по методу Сендзимира" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 14 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 15 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Перфорированный" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERSEGMENTTYPE "Кабельный лоток с соединительными деталями:DKC_G5_Sheet tray" | CABLETRAYSEGMENT | 453 occurrences
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 12 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_F5_Mesh horizontal angle:At right angles" | 11 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_F5_Mesh horizontal angle:At right angles" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TSS tapper-cover (flat):-" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>")
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TSS tapper-cover (flat):-" | 2 occurrences | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>")
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 12 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "Переход канального лотка:Переход канального лотка" | 1 occurrence | material: "<Unnamed>" | property sets: Pset_ManufacturerTypeInformation
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet reducer:-" | 1 occurrence | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_G5_Sheet horizontal bend:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 7 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 7 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TSS tapper-cover (flat):-" | 4 occurrences | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неперфорированный" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Перфорированный" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный наружный_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 9 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 23 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 7 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_TDS vertical side T-tapper:-" | 2 occurrences | material: "Предупреждение"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>")
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DDS downward vertical T-shaped tapper-cover:-" | 1 occurrence | material: materials ("<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>", "<Unnamed>")
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CDV 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот горизонтальный_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "ADSK_Поворот вертикальный внутренний_Минимальный размер:Неспецифицируемый" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 25 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DL T-tapper:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 4 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CPO 45 horizontal angle:-" | 8 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 5 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 3 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_DPT T-tapper:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 6 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 11 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CD 90 external vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_CS 90 internal vertical angle:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_Variable Angle Elbow 0-45:-" | 2 occurrences | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"
  IFCCABLECARRIERFITTINGTYPE "470_DKC_S5_RRC_RRS_RRD adapter:-" | 1 occurrence | material: "<Unnamed>"

Property sets
  Pset_BuildingStoreyCommon | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_DistributionFlowElementCommon | properties | on 3672 objects (3672 IFCFLOWFITTING)
    Reference = "OSTEC_U - ЛН, ЛП - ПШС" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 2240 objects (2240 IFCFLOWSEGMENT)
    Reference = "DKC_S5_Sheet tray" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1030 objects (1030 IFCFLOWFITTING)
    Reference = "-" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 453 objects (453 IFCFLOWSEGMENT)
    Reference = "DKC_G5_Sheet tray" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 369 objects (369 IFCFLOWFITTING)
    Reference = "Неспецифицируемый" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 68 objects (68 IFCFLOWSEGMENT)
    Reference = "DKC_G5_Ladder tray" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 45 objects (45 IFCFLOWSEGMENT)
    Reference = "По умолчанию" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 41 objects (41 IFCFLOWFITTING)
    Reference = "Неперфорированный" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon: 7 more contents on 61 objects not shown
  Pset_FlowSegmentDuctSegment | properties | on 391 objects (391 IFCFLOWSEGMENT)
    Length = 50.0000000000016 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 345 objects (345 IFCFLOWSEGMENT)
    Length = 99.9999999999989 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 269 objects (269 IFCFLOWSEGMENT)
    Length = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 220 objects (220 IFCFLOWSEGMENT)
    Length = 49.9999999999995 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 194 objects (194 IFCFLOWSEGMENT)
    Length = 100.000000000003 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 159 objects (159 IFCFLOWSEGMENT)
    Length = 49.9999999999973 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 113 objects (113 IFCFLOWSEGMENT)
    Length = 100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment | properties | on 71 objects (71 IFCFLOWSEGMENT)
    Length = 100.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentDuctSegment: 651 more contents on 1048 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 391 objects (391 IFCFLOWSEGMENT)
    Length = 50.0000000000016 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 345 objects (345 IFCFLOWSEGMENT)
    Length = 99.9999999999989 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 269 objects (269 IFCFLOWSEGMENT)
    Length = 50. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 220 objects (220 IFCFLOWSEGMENT)
    Length = 49.9999999999995 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 194 objects (194 IFCFLOWSEGMENT)
    Length = 100.000000000003 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 159 objects (159 IFCFLOWSEGMENT)
    Length = 49.9999999999973 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 113 objects (113 IFCFLOWSEGMENT)
    Length = 100. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment | properties | on 71 objects (71 IFCFLOWSEGMENT)
    Length = 100.000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_FlowSegmentPipeSegment: 651 more contents on 1048 objects not shown
  Pset_QuantityTakeOff | properties | on 3672 objects (3672 IFCFLOWFITTING)
    Reference = "OSTEC_U - ЛН, ЛП - ПШС" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2240 objects (2240 IFCFLOWSEGMENT)
    Reference = "DKC_S5_Sheet tray" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1030 objects (1030 IFCFLOWFITTING)
    Reference = "-" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 453 objects (453 IFCFLOWSEGMENT)
    Reference = "DKC_G5_Sheet tray" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 369 objects (369 IFCFLOWFITTING)
    Reference = "Неспецифицируемый" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 68 objects (68 IFCFLOWSEGMENT)
    Reference = "DKC_G5_Ladder tray" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 45 objects (45 IFCFLOWSEGMENT)
    Reference = "По умолчанию" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 41 objects (41 IFCFLOWFITTING)
    Reference = "Неперфорированный" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 7 more contents on 61 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 3708 objects (3708 IFCFLOWFITTING) | on 28 type objects
    Manufacturer = "OSTEC" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 8 (IFCINTEGER)